Share Function

- What is Share Function?

- How do I configure the Share function?

What is Share Function?

The Share Function allows logged-in subscribers to share the device on the LAN. Basically, G-4100 was a VLAN by port device, so in the default value, the users under G-4100 can not share resource to each other. This is useful for allowing subscribers to use printer and server. Topology as below.

How do I configure the Share Function?

1. In WEB GUI > Advance > Share.

2. When you select the Active/Delete/Delete All, please remember to apply the setting.

3. Notice1: The Resource IP Address must be same Subnet of LAN Subnet.

2: In Authentication mode, the subscribers must log-in the system, and then the subscriber can access the Share devices.