Firmware/Configurations Uploading and Downloading using TFTP

- Using TFTP client software
- Using TFTP command on Windows NT
- Using TFTP command on UNIX
- Downloading Walusoft TFTP from http://www.walusoft.co.uk

- Using TFTP client software

- Upload/download ZyNOS via LAN
- Upload/download SMT configurations via LAN

Using TFTP to upload/download ZyNOS via LAN

- TELNET to your P-335 Plus first before running the TFTP software
- Type the CI command 'sys stdio 0' to disable console idle timeout
- Run the TFTP client software
- Enter the IP address of the P-335 Plus
- To upload the firmware, please save the remote file as 'ras' to P-335 Plus. After the transfer is complete, the P-335 Plus will program the upgraded firmware into FLASH ROM and reboot its elf.
- To download the firmware, please get the remote file 'ras' from the P-335 Plus.

> > An example:

The 192.168.1.1 is the IP address of the P-335 Plus. The local file is the source file of the ZyNOS firmware that is available in your hard disk. The remote file is the file name that will be saved in P-335 Plus. Check the port number 69 and 512-Octet blocks for TFTP. Check 'Binary' mode for file transfering.

Using TFTP to upload/download SMT configurations via LAN

- TELNET to your P-335 Plus first before running the TFTP software
- Type the CI command 'sys stdio 0' to disable console idle timeout.
- Run the TFTP client software
- To download the SMT configuration, please get the remote file 'rom-0' from the P-335 Plus.
- To upload the SMT configuration, please save the remote file as 'rom-0' in the P-335 Plus.

> > An Example:

- The 192.168.1.1 is the IP address of the P-335 Plus.
- The local file is the source file of your configuration file that is available in your hard disk.
- The remote file is the file name that will be saved in P-335 Plus.
- Check the port number 69 and 512-Octet blocks for TFTP.
- Check 'Binary' mode for file transfering.

- Using TFTP command on Windows NT

Before you begin:

1. TELNET to your P-335 Plus first before using TFTP command
2. Type the CI command 'sys stdio 0' to disable console idle timeout

- Upload ZyNOS via LAN

`c:\tftp -i [P-335 PlusIP] put [localfile] ras`

- Download ZyNOS via LAN

`c:\tftp -i [P-335 Plus IP] get ras [localfile]`

- Upload configurations via LAN

`c:\tftp -i [P-335 Plus IP] put [localfile] rom-0`

- Download configurations via LAN

`c:\tftp -i [P-335 Plus IP] get rom-0 [localfile]`

- Using TFTP command on UNIX

Before you begin:

1. TELNET to your P-335 Plus first before using TFTP command
2. Type the CI command 'sys stdio 0' to disable console idle timeout.

Example:

`[cppwu@faelinux cppwu]$ telnet 192.168.1.1` `Trying 192.168.1.1...` `Connected to 192.168.1.1.` `Escape character is '^]'.` `Password: ****` `ras``>` sys stdio 0 `ras``> (press Ctrl+] to escape to Telnet prompt)` `telnet>` `z` `[1]+ Stopped telnet 192.168.1.1` `[cppwu@faelinux cppwu]$ tftp` `tftp``>` `connect 192.168.1.1` `tftp``>` `binary` `<- change to binary mode` `tftp``>` `get rom-0 [local-rom]` `<- download configurations` `tftp``>` `get ras [local-firmware]` `<- download firmware` `tftp``>` `put [local-rom] rom-0` `<- upload configurations` `tftp``>` `put [local-firmware] ras` `<- upload firmware`

> All contents copyright © 2006 ZyXEL Communications Corporation.