Internet Connection

A typical Internet access application of the P-335 Plus is shown below. For a small office, there are some components needs to be checked before accessing the Internet.

- Before you begin
- Setting up the Windows
- Setting up the P-335 Plus Router

- Before you begin

The P-335 Plus is shipped with the following factory default:

1. IP address = 192.168.1.1, subnet mask = 255.255.255.0 (24 b its)
2. DHCP server enabled with IP pool starting from 192.168.1.33
3. Default SMT menu password = 1234

- Setting up the Windows

1. Ethernet connection

All PCs must have an Ethernet adapter card installed.

- If you only have one PC, connect the PC's Ethernet adapter to the P-335 Plus's LAN port with a crossover (red one) Ethernet cable.
- If you have more than one PC, both the PC's Ethernet adapters and the P-335 Plus's LAN port must be connected to an external hub with straight Ethernet cable.

2. TCP/IP Installation

You must first install TCP/IP software on each PC before you can use it for Internet access. If you have already installed TCP/IP, go to the next section to configure it; otherwise, follow these steps to install:

- In the Control Panel/Network window, click Add button.
- In the Select Network Component Type windows, select Protocol and click Add.
- In the Select Network Protocol windows, select Microsoft from the manufacturers, then select TCP/IP from the Network Protocols and click OK.

3. TCP/IP Configuration

Follow these steps to configure Windows TCP/IP:

- In the Control Panel/Network window, click the TCP/IP entry to select it and click Properties button.
- In the TCP/IP Properties window, select Obtain an IP address automatically.

Note: Do not assign arbitrary IP address and subnet mask to your PCs, otherwise, you will not be able to access the Internet.

- Click the WINS configuration tab and select Disable WINS Resolution.
- Click the Gateway tab. Highlight any installed gateways and click the Remove button until there are none listed.
- Click the DNS Configuration tab and select Disable DNS.
- Click OK to save and close the TCP/IP properties window
- Click OK to close the Network window. You will be prompted to insert your Windows CD or disk. When the drivers are updated, you will be asked if you want to restart the PC. Make sure your P-335 Plus is powered on before answering Yes to the prompt. Repeat the above steps for each Windows PC on your network.

- Setting up the P-335 Plus Router

The following procedure is for the most typical usage of the P-335 Plus where you have a single-user account (SUA). The P-335 Plus supports embedded web server that allows you to use Web browser to configure it. Before configuring the router using Browser please be sure there is no Telnet or Console login.

1. Retrieve P-335 Plus Web

Please enter the LAN IP address of the P-335 Plus router in the URL location to retrieve the web screen from the P-335 Plus. The default LAN IP of the P-335 Plus is 192.168.1.1. See the example below.

2. Login first

To restrict only the adminstrator can configure the router, there is a login procedure prompted for asking User Name and Password. The default User Name is 'admin' and the default password is the default SMT password, '1234'.

3. Configure P-335 Plus for Internet access by using WIZARD SETUP. The Web screen shown below takes PPPoE as the example.

Key Settings:

Option | Description
Encapsulation | Select the encapsulation type your ISP supports
Service Name | Enter the 'Service Name' for the ISP
User Name | Enter the login user name given by the ISP
Password | Enter the password given by the ISP
Idle Timeout | This value specifies the time in seconds that can elapse before the P-335 Plus automatically disconnects the PPPoE connection.

4. WAN IP Address Assignment

Check 'Get automatically from ISP' if the ISP provides the IP dynamically, otherwise check 'Use fixed IP address' and enter the static IP in the 'IP Address' field.

5. Check if the connection is up by clicking the ADVANCED/MAINTENANCE menu.

All contents copyright (c) 2006 ZyXEL Communications Corporation.