LAN-To-LAN Connection Wizard - Client Setup Client Setup This screen is to enter the information of your Prestige 681 acts as a client required for LAN-To-LAN connection.
Description
Link Compatibility: Select the SDSL router type that your SDSL is compatible. Currently, P681 supports Ascend/Lucent and Copper Mountian only. Transfer Rate: For Ascend/Lucnt SDSL router type, please select the matching transmission speed of peer. For Copper Mountian SDLSL router type, the rate will be set as Auto. Frame Relay Option: This function is responsible for monitoring the up/down status and error performance of an individual link. If failure occurs, it also initiates recovery actions for the restoration of the failed link. For North American switches, this field should be set to ANSI. Set to ITU-T for switches outside North America. Then, click Next to go to next step for the ISP configuration of router.

ZyXEL Communications Corporation