LAN-To-LAN Connection Wizard - Remote Node Setup Remote Node Setup This screen is to enter the information of your Prestige 681 for LAN-To-LAN Connection.
Description
Remote IP Address: Enter the IP address of the remote gateway. To have a correct IP address, you have to fill in either the remote Prestige WAN IP address or the remote Prestige LAN IP address depending on the remote WAN IP settings. DLCI(Data Link Connection Identifier): The carrier gives you a specific DLCI for each PVC which is a path number of a portion of the PVC, not the address of the destination. WAN Port TCP/IP Encapsulation: Enter the encapsulation information that needed for the connection My Login Name: Enter the login name that needed for the connection. My Password: Enter the password associated with the login name above. Then, click Finish to save the configuration to router.

ZyXEL Communications Corporation