Internet Access Wizard - ISP Setup ISP Setup This screen is to enter the account information of your ISP required for Internet access. The information is provided from your ISP when you applied the account. The following information will help you to understand how to fill up the settings in this screen.
Description
My ISP Select your ISP from the list, most default values will be set automatically. For example, if you select "Bell Atlantic" in the list, the VPI will be set as 0 and the VCI will be set as 35. Protocol Enter the encapsulation information that your ISP gave you. Virtual Circuit ID VPI: Enter the Virtual Path Identifier(VPI) that your telephone company supplies. VCI: Enter Virtual Channel Identifier(VCI) that your telephone company supplies. WAN Port TCP/IP Service Name: This is valid only when you have chosen PPPoE encapsulation. If you are using PPPoE encapsulation, then type the name of your PPPoE service here. User Name: Enter the login name that your ISP gives you. Password: Enter the password associated with the login name above. ENET ENCAP Gateway: ENET ENCAP requires that you specify a gateway IP address in this field. Enter the gateway IP address supplied by your ISP if applicable. WAN IP Address: Enter the IP address supplied by your ISP if applicable. Then, click Exit to save the configuration to router.
More
Click on the fields in the image below to go to the appropriate description.
Description
Ethernet TCP/IP Setup IP Address and Subnet Mask: The Prestige is pre-configured in the factory with an IP address of 192.168.1.1 and a subnet mask of 255.255.255.0 (class C). This combination should work fine for the majority of cases. Leave them as is if your ISP did not explicitly assign you any IP address for your LAN. Otherwise, select one from the assigned addresses that is easier to remember for your Prestige. The PNC will compute the subnet mask automatically based on the IP address that you assign to the Prestige. Do not change the computed value unless your ISP tells you to do so. DNS Server Address DNS (Domain Name System) is for mapping a domain name to its corresponding IP address and vice versa, e.g., the IP address of www.zyxel.com is 204.217.0.2. The DNS server is extremely important because without it, you must know the IP address of a machine before you can access it. The DNS server addresses that you enter in the DHCP setup are passed to the client machines along with the assigned IP address and subnet mask. Make sure that you obtain the IP address of the DNS server(s) from your ISP. Your workstations will need this information even if you don't use the Prestige's DHCP server.

ZyXEL Communications Corporation