Prestige Login Change Prestige's IP Address The default IP address of ZyXEL Prestige is 192.168.1.1. While starting PNC, the program will detect the IP address and the subnet mask for your PC. Before configuring your Prestige with PNC, make sure that the IP address and the subnet mask for your Prestige are in the same range as your PC's IP; otherwise, the program will ask you to either change the IP address/subnet mask for your Prestige or change the IP address/subnet mask for your PC as shown in the following image.
To change the IP address/subnet for your Prestige, enter the appropriate IP address/subnet mask into the text boxs, then click OK to configure your Prestige. Then, the program will bring you the screen of Internet Access Wizard. To change the IP address/subnet for your PC, select 'No, I will not change them,' click OK to exit this program, then use the Network control panel to change for your PC. Login to Your Prestige If you have more than one ZyXEL Prestige router connecting with your PC, the Prestige router found will be listed in the middle box as shown in the image below. The information for your Prestige router includes Name, Model, IP Address and MAC address. You can only choose one to make connection for one time.
Click on the fields in the image below to go to the appropriate description.
Description
Fresh: Refresh Prestige list box. Password: Enter the system password to log in to your Prestige router, then click on Login button. Your Prestige is shipped with a default system password of 1234. Login: After entering the system password, click this button to login. Cancel: Exit ZyXEL Prestige Network Commander program.

ZyXEL Communications Corporation